Reset Gigaset BASE station to Factory defaults: N510, N720

1. Turn off the device.
2. Hold down the **“Connect”** button on the base.

A picture containing graphical user interface

Description automatically generated

1. Power on the device while keeping the **“Connect”** button pressed and wait 15 seconds until the **“Connect”** button start to blink fast.
2. Release the **“Connect”** button and power off the device.
3. Your DECT system has been successfully reset

Reset Gigaset Handsets to Factory defaults: R650H Pro

1. Press the **“Menu”** key.

A picture containing text, monitor, electronics, cellphone

Description automatically generated

1. Navigate to **“Settings”** → **“System”** → click **“Yes”** to reset settings.